
Control and Smart Control main board replacement instructions


Included tools:




1. Remove main housing (T-20 bit)




1. With covers removed, main board is exposed



1. Unplug the 4 cords from the board



1. Remove the three screws



1. Install the new board by reversing these steps.
2. Reinstall covers

NOTE: CONTROL TRAINERS ONLY HAVE 3 WIRES. SMART CONTROL TRAINERS (SHOWN HERE) HAVE 4 WIRES.

Be sure to pair with the Kinetic Fit app and update firmware immediately after board installation.